	

ПРИЛОЖЕНИЕ №1 КЪМ ПОКАНАТА 



ТЕХНИЧЕСКО ЗАДАНИЕ
ЗА „АБОНАМЕНТНО ОБСЛУЖВАНЕ НА СИСТЕМА ЗА ВИДЕО КОНТРОЛ, ИНСТАЛИРАНА НА ЛЕТИЩЕ СОФИЯ”



1. Обхват на поръчката 

Системата за видео контрол, инсталирана на летище София включва:видеокамери, монитори, архиватори, компютри, захранващи устройства и други, както следва:

Терминал 1
	№
	Наименование
	Модел / Произв.
	Бр.

	1
	Монитор 24’
	Samsung
	2

	2
	Монитор 19’
	LOC
	6

	3
	Монитор 21,5’
	LOC
	2

	4
	Монитор 43’
	LG
	4

	5
	Статична камера
	Panasonic/Samsung
	155

	6
	Видео рекордер – DVR 16
	Instek
	6

	7
	Видео рекордер – DVR 32
	Instek
	1

	8
	Видео рекордер – DVR 16
	Hikvision
	2

	10
	Видео рекордер – DVR/NVR хибриден 
	DH-XVR5232ANX
	2

	11
	Оптичен видео конвертор
	Wintoptec
	10

	12
	Мрежов комутатор
	Cisco
	2

	13
	Команден център
	Instek
	2

	14
	Персонален компютър със спец. софтуер
	
	2



Терминал 2
	№
	Наименование
	Модел / Произв.
	Бр.

	1
	Алармено устройство 64 входа/ 8 изхода
	LCT 8504/00
	1

	2
	Разделящо устройствобош с пулта за управление
	LCT 8568/00 
	1

	3
	Основен превключвател
	LCT 8944/92
	1

	4
	Резервен превключвател
	LCT 8945/92 
	1

	5
	Процесорно устройство
	LCT 8901/50 
	1

	6
	безична клавиатура
	KBD Universal   
	4

	7
	Статична камера
	LCT 0455/50 
	275

	8
	Управляема камера
	LCT 0455/51
	16

	9
	Вътрешна камера DOME
	Q3ATPW5TP
	13

	10
	Детектори за движение
	YMD-11
	128

	11
	Захранване
	PSU 515R
	16

	12
	Медиен конвертор
	S700VT
	88

	13
	Медиен конвертор
	S732DVT
	40

	14
	Медиен конвертор
	S732DVR
	68

	15
	Медиен конвертор
	S702VT-RST
	60

	16
	Медиен конвертор
	S702VT
	43

	17
	Медиен конвертор
	S702VR-RST2
	43

	18
	1/2" Zoom обектив 
	LTC 3293/30
	16

	19
	1/3" Zoom обектив 
	LTC 3394/50
	12

	20
	Обективи за статични камери
	LTC 3364/60
	86

	21
	Архиватори
	Instek
	12

	22
	Команден център
	Instek
	3

	23
	Монитори 43’
	Crown
	4

	24
	Монитори 42’
	Panasonic
	4

	25
	Монитори 19’
	LG
	41

	26
	Монитори 43’	
	LG
	2







Обществен платен паркинг Т1 и Т2, регистриране ДКН автомобили и служебен паркинг Т1

	№
	Наименование
	Модел / Произв.
	Бр.

	1
	IP камера
	Honeywell
	29

	2
	IP камера
	Hikvision
	68

	3
	Видео рекордер NVR16 входа
	Hikvision
	5

	4
	Видео рекордер NVR 32входа
	Dahua
	1

	5
	Персонален компютър със спец. софтуер „Аутомаршал“
	Lenovo
	1

	6
	Персонален компютър със спец. софтуер
	Deluxe Asus
	1




Демаркирана зона на правителствен VIP А, мост „Север-юг”, ГРП и ПП №5 – северен район
	№
	Наименование
	Модел / Произв.
	Бр.

	1
	Стационарна камера
	Hikvision
	25

	2
	Захранващ блок
	Wintech
	1

	3
	Термовизиона камера
	
	2

	4
	Видео рекордер – DVR 
	Hikvision
	4




АУЦ 
	№
	Наименование
	Модел / Произв.
	Бр.

	1
	Стационарна камера
	Panasonic
	4

	3
	Стационарна камера
	Hikvision
	6

	5
	Видео рекордер – DVR
	Hikvision
	1




Разтоварище ГСМ, ГСМ и автостопанство 
	№
	Наименование
	Модел / Произв.
	Бр.

	1
	Стационарна камера
	Hikvision
	2

	2
	IP камера
	Hikvision
	10

	3
	Видео рекордер – DVR 
	Hikvision
	1

	4
	Видео рекордер - NVR
	Hikvision
	1

	5
	Персонален компютър със спец. софтуер
	HP
	2

	6
	Енкодер 4 входа
	Hunt
	1



ЦИК
	№
	Наименование
	Модел / Произв.
	Бр.

	1
	Видео рекордер - DVR
	Panasonic
	1

	2
	Стационарна камера
	Panasonic
	2

	3
	PTZ камера
	Panasonic
	1

	4
	Оптичен видео конвертор
	Wintoptec
	2

	5
	Монитор 21’
	ЛОС
	1

	6
	1/2" Zoom обектив
	Panasonic
	1

	7
	IP камера
	Dahua
	6

	8
	Видео рекордер - NVR
	Dahua
	1



2. Описание и обхват на дейностите, включени в абонаментното обслужване:
2.1. Абонаментното обслужване за период от 12 (дванадесет) месеца на системата за видеоконтрол на летище София, включва извършването на профилактика и диагностика – преглед, тестване и пускане в експлоатация след тестването, осигуряване на пълната работоспособност и функционалност на системата във вида и обема от компоненти, модули, услуги, версии на съответните софтуери и продукти и др., в последователност съгласно инструкциите за експлоатация на системите и компонентите. Минимално необходимите дейности за извършване на задължителна профилактика и диагностика включват:
· Предварителен основен преглед на всички журнални файлове на системата за наличие на събития и процеси извън нормалната работа на системата;
· Архивиране на основната база на системата;
· Стартиране на вградените в системата основни тестови процедури, наблюдение и анализ на резултатите от тестовете;
· Основен преглед на работоспособността на всички модули, платки и компоненти на системата и съответна подмяна на дефектирали такива.
Профилактиката и диагностиката на системата се извършва минимум един път месечно. Минималните дейности, които Изпълнителят е длъжен да извърши при посещението си, както и дейностите по техническа поддръжка, са подробно описани в Техническата спецификация. Независимо от това Изпълнителят има задължението да идва на място в случай на възникване на аварийни ситуации или друг вид дейности, необходими за осигуряването на нормалното функциониране на системата за видеоконтрол, като посещението е включено в месечната цена за абонаментно обслужване и не се заплаща допълнително.
2.2. Абонаментната  поддръжка на системата за видеоконтрол инсталирана на летище София за период от 12 (дванадесет) месеца включва: сервизиране, настройки и почистване на всички електронни модули, посочени в Приложение 1;
          2.3.  Време за отстраняване на възникнал проблем – до 24 часа от уведомлението от „СОФ Кънект“ АД в случай, че частите са налични за влагане към момента на уведомлението.
          2.4. Поддръжка от страна на Изпълнителя на денонощна телефонна линия за техническа поддръжка;
          2.5.  Консултации по телефона или на място – по всяко време в рамките на работния ден.


      
	

APPLICATION 1


SPECIFICATIONS
FOR "SUBSCRIPTION SERVICE OF A VIDEO CONTROL SYSTEM INSTALLED AT SOFIA AIRPORT"




1. Scope of the order

The video surveillance system installed at Sofia Airport includes: video cameras, monitors, archivers, computers, power supplies and others, as follows:

Terminal 1

	№
	Name
	model
	Pc.

	1
	Monitor 24’
	Samsung
	2

	2
	Monitor 19’
	LOC
	6

	3
	Monitor 21,5’
	LOC
	2

	4
	Monitor 43’
	LG
	4

	5
	Fixed camera
	Panasonic/Samsung
	155

	6
	Video recorder – DVR 16
	Instek
	6

	7
	Video recorder – DVR 32
	Instek
	1

	8
	Video recorder – DVR 16
	Hikvision
	2

	10
	Video recorder – DVR /NVR hybrid
	DH-XVR5232ANX
	2

	11
	Optical  video converter
	Wintoptec
	10

	12
	Network switch
	Cisco
	2

	13
	Command center
	Instek
	2

	14
	Personal computer with special software
	Instek
	2


















Terminal 2
	№
	Name
	Model
	Pc.

	1
	Alarm device 64 inputs / 8 outputs
	LCT 8504/00
	1
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	Bosch splitter with control panel
	LCT 8568/00 
	1

	3
	Main switch
	LCT 8944/92
	1

	4
	Spare switch
	LCT 8945/92 
	1

	5
	Processor device
	LCT 8901/50 
	1

	6
	Wireless keyboard
	KBD Universal   
	4

	7
	Fixed camera
	LCT 0455/50 
	275

	8
	Controlled camera
	LCT 0455/51
	16

	9
	Internal camera
	Q3ATPW5TP
	13

	10
	Motion detectors
	YMD-11
	128

	11
	Power supply
	PSU 515R
	16

	12
	Media converter
	S700VT
	88

	13
	Media converter
	S732DVT
	40

	14
	Media converter
	S732DVR
	68

	15
	Media converter
	S702VT-RST
	60

	16
	Media converter
	S702VT
	43

	17
	Media converter
	S702VR-RST2
	43

	18
	1/2" Zoom lens 
	LTC 3293/30
	16

	19
	1/3" Zoom lens 
	LTC 3394/50
	12

	20
	Lenses for Fixed cameras
	LTC 3364/60
	86

	21
	Archivers
	Instek
	12

	22
	Command center
	Instek
	3

	23
	Monitors 43’
	Crown
	4

	24
	Monitors 42’
	Panasonic
	4

	25
	Monitors19’
	LG
	41

	26
	Monitors43’	
	LG
	2







Public paid parking T1 and T2, car registration/ID number


	№
	Name
	Model
	Pc.

	1
	IP camera
	Honeywell
	29

	2
	IP camera
	Hikvision
	68

	3
	Video recorder NVR 16 entrance
	Hikvision
	5

	4
	Video recorder NVR 32 entrance
	Dahua
	1

	5
	Personal computer with special software "Auto Marshal"
	Lenovo
	1

	6
	Personalcomputer with special software
	Deluxe Asus
	1




Demarcated zone of government VIP A, bridge "North-South", BCP/border crossing point and checkpoint№5 - northern region
	№
	Name
	Model
	Pc.

	1
	Stationary camera
	Hikvision
	25

	2
	Power supply 
	Wintech
	1

	3
	Thermal imaging camera
	
	2

	4
	Video recorder - DVR
	Hikvision
	4




Aviation Training Center
	№
	Name
	Model
	Pc.

	1
	Stationary camera
	Panasonic
	4

	3
	Stationary camera
	Hikvision
	6

	5
	Video recorder - DVR
	Hikvision
	1




GCP/ Gas control pointunloading fuels and lubricants
	№
	Name
	Model
	Pc.

	1
	Stationary camera
	Hikvision
	2

	2
	IP camera
	Hikvision
	10

	3
	Video recorder - DVR
	Hikvision
	1

	4
	Video recorder - NVR
	Hikvision
	1

	5
	Personal computer with special software
	HP
	2

	6
	Encoder 4 entrance
	Hunt
	1




Coordination center
	№
	Name
	Model
	Pc.

	1
	Video recorder - DVR
	Panasonic
	1

	2
	Stationary camera
	Panasonic
	2

	3
	PTZcamera
	Panasonic
	1

	4
	Optical video converter
	Wintoptec
	2

	5
	Monitors21’	
	ЛОС
	1

	6
	1/2" Zoom lens 
	Panasonic
	1

	7
	IP camera
	Dahua
	6

	8
	Video recorder - NVR
	Dahua
	1



2. Description and scope of the activities included in the subscription service:
2.1. The subscription service for a period of 12 (twelve) months of the video surveillance system at Sofia Airport includes the performance of prophylaxis and diagnostics - inspection, testing and commissioning after testing, ensuring the full operability and functionality of the system in the form and volume of components, modules, services, versions of the respective software
products, etc., in sequence according to the operating instructions of the systems and components. The minimum necessary activities for mandatory prevention and diagnosis include:

• Preliminary basic overview of all log files of the system for the presence of events and processes outside the normal operation of the system;
• Archiving of the main base of the system;
• Starting the basic test procedures built into the system, monitoring and analysis of test results;
• Basic inspection of the operability of all modules, boards and components of the system and appropriate replacement of defective ones.

The prevention and diagnostics of the system is performed at least once a month. The minimum activities that the Contractor is obliged to perform during his visit, as well as the technical support activities, are described in detail in the Technical Specification. Nevertheless, the Contractor has the obligation to come on site in case of emergencies or other activities necessary to ensure the proper functioning of the video surveillance system, as the visit is included in the monthly price for subscription service and is not paid extra.


2.2 The subscription support of the video surveillance system installed at Sofia Airport for a period of 12 (twelve) months includes: servicing, settings and cleaning of all electronic modules listed in Annex 1;
2.3. The deadline for elimination of problems occurred with a video surveillance system – up to 24 hours from the notification by SOF Connect AD in case there are spare parts available at the time of notification;
2.4. Round the clock „emergency phone“ line for technical support;
2.5. Consultations over the phone or on site - at any time during working days.
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