Slot Coordination for General / Business Aviation 
1. GCR Standard format

The GCR standard request consists of 3 main components.
 
GCR                                   


/FLT      1. Message Header

LBSF



NABC123 08JUN 010G159 LSZH0900 D        

N ABC456 09JUN 010G159 1200LSZH D       


SI IF NOT AVBL PLS CFM NEXT LATER POSS      


GI BRGDS ...........

1.1. Header 

GCR
Type of request: GCR - General aviation Clearance Request


/FLT
Message type for operation using flight designator plus flight number or the aircraft                     
                         registration
FLT  = Slot request  using flight number or call sign    .
REG = Slot request using aircraft registration.

LBSF
Airport at which slots are being requested: ICAO code
1.2.  Flight details lines
The flight detail lines contain all of the  necessary schedule information needed to request an airport slot. The following examples show the different format required to request either an arrival or departure slot.
1.2.1. Arrival Slot Format

NABC123 08JUN 010G159 LSZH0900 D






For an arrival slot, the registration or flight number comes directily, that is to say without a space, after the action code.
The scheduled time of arrival (STA) comes directly, that is to say, without a space, after the airport of origin.
1.2.2. Departure Slot Format

N ABC456 09JUN 010G159 1200LSZH D   

For a departure slot, a space MUST comes between the action code and the registration, respectively, the flight number.

The scheduled time of departure (STD) comes directly, that is to say, without a space before  the destination airport.
Action Code 
The action code defines the exact intention of the GCR sender and is always at the beginning of the line. According to the sender, following codes are possible in the GCR format:
	     GCR Action Codes 

	

	     Owner / Operator
	     Coordinator

	
	

	 
	 

	     N New schedule 
	     K Confirmation

	     D Delete schedule
	     X Cancellation

	     C Schedule to be changed
	     H Holding

	     R Revised schedule
	     U Refusal

	 
	     W Wrong 


Registration / Flight number
Both registration and flight number are possible. (Reference is made in the   

corresponding message header). A flight number combines a maximum of 7 letters and 

digits (2-3 letters followed by 1-4 digits with an optional letter as a suffix).

Date of Operation
            The date of operation refers to the scheduled UTC departure and arrival times at the airport to   
            be coordinated.
Aircraft Type
Information referring to the type of aircraft being used consists of: 

– Number of seats (3 digits)

– Aircraft type in ICAO format (4 letters)

Number of seats and aircraft type are entered without a space in between.

Routing and Time of Flight
– Routing information consists of the origin or destination airport in regard to the airport being coordinated.
– The requested arrival or departure time at the airport being coordinated, is stated in UTC.
Routing information and the requested timing are not separated by a space.
Type of Flight  
One of the following service type codes can be used to define the flight:
“ N “ 
Business Aviation / Air taxi

“ D ”
General Aviation 

“ I  “ 
State / Diplomatic flight
“ U “     Air Ambulance / Humanitarian flight

“ E “
Government flight
            “ W “
Military flight

“ E “
Government flight 

“ P “
Positioning / Ferry flight without passengers
            “ K “
Crew training / School

            “ X “
Technical stop 

            “ T “
Technical test
1.3. Footnote
SI – Special Information  (eg. IF NOT AVBL PLS CFM NEXT LATER POSS)
GI – General Information ( eg. BRGDS) 

2. GCR Examples
2.1.  Airport Slot Request 
Example.1N :
Slot request for  a departure flight using a registration (Action code “N”)




Airport being coordinated :
LBSF
Type of Aircraft :
Gulfstream G-159
Registration HBIEV

Flight details :    
Departure:
  LBSF

0750utc / 08JUN






             Arrival: 
              LOWW
0900utc / 08JUN



GCR

/REG

LBSF
N HBIEV 08JUN 010G159 0750LOWW D

GI BRGDS ……………  

----------------------------------------------------------------------------------

Example.2N :
Slot request for an arrival using a flight number or a call sign (Action code  “N”)


Airport being coordinated:
LBSF
Type of Aircraft :
Gulfstream G-159
Flight number: ABC123

Flight detail:       
Departure:
  LSZH

0750utc / 08JUN





             
Arrival:                LBSF   
0900utc / 08JUN






 
GCR

/FLT

LBSF
NABC123 08JUN 010G159 LSZH0900 D

GI BRGDS ……………  

----------------------------------------------------------------------------------

Example.3N :
Slot request for  an arrival and departure with differing flight numbers or call signs.
                         (Action code “N”)


Airport being coordinated:    LBSF
Type of aircraft:   
Gulfstream G-159

Flight information:  Departure:LSZH
0750utc / 08JUN      Flight number:ABC123




    Arrival:       LBSF
0900utc / 08JUN






    Departure:  LBSF
1200utc / 09JUN      Flight number: ABC456





    Arrival:       LSZH
1310utc / 09JUN



GCR

/FLT

LBSF
NABC123 08JUN 010G159 LSZH0900 D

N ABC456 09JUN 010G159 1200LSZH D

GI BRGDS ……………  

-----------------------------------------------------------------------------------
2.1.1. 
Possible replies from the coordinator
            The coordinator’s replies are also in the GCR standard format as described above.

            The only difference is in the use of the “action code.” 
Example.1NA :
 The requested airport slots in examples 1N, 2N and 3N have been allocated 
(Action code „K“)

GCR

/REG

LBSF
K HBIEV 08JUN 010G159 0750LOWW D

GCR

/FLT

LBSF
KABC123 08JUN 010G159 LSZH0900 D

            GI BRGDS ……………  
GCR

/FLT

LBSF
KABC123 08JUN 010G159 LSZH0900 D

K ABC456 09JUN 010G159 1200LSZH D

GI BRGDS ……………  
Example.2NA:
The requested airport slots in examples 1N, 2N and 3N  are not available. 
(Action code ”U”)

                         The nearest available slots have been allocated.

GCR

/REG

LBSF
U HBIEV 08JUN 010G159 0750LOWW D

K HBIEV 08JUN 010G159 0810LOWW D

GI BRGDS ……………
GCR

/FLT

LBSF
UABC123 08JUN 010G159 LSZH0900 D

KABC123 08JUN 010G159 LSZH0920 D

GI BRGDS ……………  

GCR

/FLT

LBSF
UABC123 08JUN 010G159 LSZH0900 D

KABC123 08JUN 010G159 LSZH0920 D

U ABC456 09JUN 010G159 1200LSZH D

K ABC456 09JUN 010G159 1200LSZH D

GI BRGDS ……………  
--------------------------------------------------------------------------------------
2.2. Cancellation of cleared slots 
If a cleared slot is to be cancelled, it is important to make sure that the flight details are identical with the  originally cleared airport slot. If this is not the case, the cancellation request can not be processed.
Example. 1D:
Slots allocated in example 3N are to be cancelled. (Action code “D”)

GCR
/FLT

LBSF
D ABC123 08JUN 010G159 0500EDDL D 
DABC124 08JUN 010G159 EDDF0550 D 
GI BRGDS ……………  

--------------------------------------------------------------------------------------
2.2.1. Replies from the coordinator 
Example1DA:
The cancellation of slots in example 1D is confirmed. (Action code “X”)

GCR

/FLT

LBSF
X ABC123 08JUN 010G159 0500EDDL D 
XABC123 08JUN 010G159 EDDF0550 D 
GI BRGDS ……………
--------------------------------------------------------------------------------------
2.3. Changing a cleared slot  
Flight details can be changed by using a combination of the action codes “C” and “R”.
The C line defines the existing slot clearance originally allocated by the coordinator and the “R” line  defines the new slots details requiring slot clearance. It is important to make sure that the flight details in the C line are identical with the originally allocated and confirmed airport slot.
Example.1C:
Time change
Type of Aircraft:
  Gulfstream G-159
Registration: HBIEV

Flight details:    Departure:    LBSF
 1200utc iso 0750utc / 08JUN
    




            Arrival:          LOWW   
 1310utc iso 0900utc / 08JUN




GCR

/REG

LBSF
C HBIEV 08JUN 010G159 0750LOWW D 
R HBIEV 08JUN 010G159 1200LOWW D

GI BRGDS ……………  

--------------------------------------------------------------------------------------
Example.2C:
Change in date / time / arrival airport

Type of Aircraft:
Gulfstream G-159
Registration HBIEV

Flight details:    Departure:    LBSF
 0600utc iso 0750utc / 09JUN iso 08JUN
    




             Arrival:         LSZH   
 1310utc iso 0900utc / 09JUN iso 08JUN      

GCR

/REG

LBSF
C HBIEV 08JUN 010G159 0750LOWW D 
R HBIEV 09JUN 010G159 1200LSZH D

GI BRGDS ……………  

--------------------------------------------------------------------------------------
2.3.1.

Possible replies from the coordinator  
Example.1CA:
 The time change in example 3C is confirmed. (Action code “K”)
                          The original slots are cancelled simultaneously. (Action code “X”)

GCR

/REG

LBSF

X HBIEV 08JUN 010G159 0750LOWW D 
K HBIEV 09JUN 010G159 1200LSZH D

GI BRGDS …………… 

--------------------------------------------------------------------------------------
Example.2CA:
The slots requested in example 3C are not available. (Action code “U”)

                          The nearest available alternative slots are allocated (Action code “K”) and the    

                          original slots are simultaneously cancelled. (Action code “X”)
GCR

/REG

LBSF

X HBIEV 08JUN 010G159 0750LOWW D 
U HBIEV 09JUN 010G159 1200LSZH D

K HBIEV 09JUN 010G159 1220LSZH D

GI BRGDS ……………
--------------------------------------------------------------------------------------
Type of flight





Type of flight





Number of seats + aircraft type (ICAO)





Scheduled time of departure (UTC) + destination airport(ICAO)





Date of operation





Registration of flight number, respectively, call sign





Number of seats + aircraft type (ICAO)





Action Code





Origin of flight  (ICAO) + scheduled time of  arrival  (UTC)





Date of operation





 Registration or flight number, respectively, call sign





 Action Code





3. Footnotes





2. Flight details line(s)
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